**Additional Components Chart for:**

**Fontanot Eureka Spiral Staircase Kit**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  |  | |  | **Additional Components Required** | | |
|  | | **Staircase Height in cm** | | **Rises** | Additional Treads | Shorter Centre Pole | Additional Handrail |
|  | | **EU Regs** | **UK Regs** |  |  |  |  |
|  | | 336-376 | 336-352 | 16 | +3 | +1 | - |
|  | | 315-352 | 315-330 | 15 | +2 | +2\* | - |
|  | | 294-329 | 294-308 | 14 | +1 |  | - |
| STANDARD KIT | | 273-305 | 273-286 | 13 | **Standard Kit with 12 treads + 1 landing tread** | | |
|  | | 252-282 | 252-264 | 12 |  |  |  |
|  | | 231-258 | 231-242 | 11 |  | +1\* |  |
|  | | 210-235 | 210-220 | 10 |  | +1\* |  |
|  | |  |  |  |  |  |  |
|  | | Tread rise is adjustable from 21.0 to 23.5cm | |  | \*replaces the existing 125cm pole included in the kit | | |
|  | | Maximum tread rise is 22cm for dwellings to UK Regs | | Please note that it is your responsibility to determine if your installation is subject to the Building Regulations. If you would like advice, please feel free to contact our team to discuss your project – 08456 210193. | | | |